* **Current fire station built in 1952**
  + **Smaller fire trucks / no vehicle maintenance area**
    - New trucks taller and wider / 12 ft high x 8 ½ ft wide / 2 vehicles currently stored in tents
    - Current doors 11 feet / new doors 14 feet
    - 6 bays for current apparatus and maintenance
    - Engine 2,4,5,6 / Ladder 1,2 / Squad 1,2 / Fire Alarm / Car 2 / Boat
  + **Insufficient diesel exhaust removal system / not provided for all vehicles**
    - Plymo vent system will be provided for all vehicles
    - Vehicle exhaust will be restricted to apparatus bays
    - Also, proper storage for PPE / 2 sets / off gases for 4 hours
  + **No administrative space / administrative assistant / fire prevention**
    - Administrative assistant office
    - Fire prevention office / plan review / issue permits
    - Office space / training, ems, medical, arson investigation
  + **Insufficient living quarters / no accommodations for female firefighters**
    - Two person dormitories / extra accommodations for emergency hold overs
    - Female dormitories and locker room
    - Fire officers dorm / office / incident reports
  + **Unhealthy building / no HVAC / firefighter illness in winter**
    - New HVAC
  + **No public restroom facilities**
    - Will be provided in lobby and fire station / ADA compliant
  + **No training facilities**
    - Shared training room / Mass. Fire Academy classes 35-50 seats
    - EMS weekly training
    - Joint training classes
    - LEPC / REPC training exercises
  + **Emergency operation center / currently in Town Hall / insufficient facilities**
    - Emergency Operations Director is responsible for EOC
    - Training room also serves as EOC and community room